This folder contains the data used in the manuscript titled: Solid-state-biased coherent detection of ultra-broadband terahertz pulses.
FIRST GENERATION
In the folder “First generation” we report the data acquired with the first generation detectors.
The folder contains 12 files. The file name indicates the width of the slit (30 microns) and the applied voltage (from 500V to 5000V), and the letter t and E, shows time and electric field.
The vector named “t” contains the time-axis information for the acquisition. The units are seconds.
The vector named “E” contains the electric field corresponding to t for that acquisition.
ABCD REFERENCE
The folder named ABCD reference contains the time axis in seconds (ABCD_reference_2_5kV_100ms_600ms_500Hz_t) and the normalised electric field values (ABCD_reference_2_5kV_100ms_600ms_500Hz_E) for a measurement taken with ABCD detection, using 2.5kV bias, 100ms time constant on the lock in, and chopping at 500 HZ.
SECOND GENERATION
This folder contains four folders. Each of the four folders contains the electric field recordings for different detector parameters. These parameters are stated in the sub-folder name. For example “10um_finger_3um_gap_100ms_500Hz “ includes electric field traces acquired with a sensor having a 10-micrometre width finger, 3-micrometre width gap, acquisition performed with 100ms time-constant on the lock-in, and 500Hz chopping frequency. 
Inside each sub-folder, the files are named according to the bias field applied, t indicates the time axis (in seconds) and E shows the Electric field amplitude (according to the lock-in, i.e., uncalibrated).
IBUPROFEN
This folder contains the reference (Ref) and the sample (Ibu) acquisition for the Ibuprofen study. The file name is indicative of the lock-in time constant and chopping frequency.
EOSvsSSBCD
This folder contains the acquisition of the electric field trace via SS-BCD and electro-optical sampling. The name of the files indicates the lock-in time constant and optical power.