The files for the multichannel version of the composition Image 8 are included in the folder, ‘Image 8 - Multichannel Audio Files’. The discrete multichannel files are named as follows:
 
1. Image 8 (4.1) - L.wav
2. Image 8 (4.1) - R.wav
3. Image 8 (4.1) - Rs.wav
4. Image 8 (4.1) - Ls.wav
5. Image 8 (4.1) - LFE.wav
6. Image 8 (Ambisonic - 1st Order FuMa).aif
 
At the time of writing this, this piece can be play back using various software, but a relatively simple way is via a Digital Audio Workstation (DAW), assigning each of the above tracks to individual speakers:
 
1. Image 8 (4.1) - L.wav should be assigned to the front left speaker.
2. Image 8 (4.1) - R.wav should be assigned to the front right speaker.
3. Image 8 (4.1) - Rs.wav should be assigned to the rear right speaker.
4. Image 8 (4.1) - Ls.wav should be assigned to the rear left speaker.
5. Image 8 (4.1) - LFE.wav should be assigned to a subwoofer.
6. You will also require an Ambisonic decoder to play back the ‘Image 8 (Ambisonic - 1st Order FuMa).aif’ file. Otherwise, it won’t play back as intended. Look online (or elsewhere) to determine how to play back a FuMa Ambisonic file in the DAW, or other playback software, you are using.
 
Ensure all the speakers are equidistant from each other and that they have been calibrated so the audio from each is at the same volume.