Dataset for Fiber-coupled superconducting nanostrip single-photon detector with blackbody-limited performance from the near to mid-infrared


This is a dataset for characterisation of a impedance matched, differentially biased W0.5Si0.5 SNSPD with an active area of 23 x 24 um and an optical cavity with maximal absorption at 2.9 um.


Please refer to the manuscript and supplementary information for further context or feel free to email daniel.kuznesof@gmail.com for further clarification.