CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.6.4/conf/instr/spect/uxnmr.info
Date         : Thu Mar 17 14:10:00 2022
Release      : TopSpin 3.6.4
Installed in : /opt/topspin3.6.4
Host         : benmore
OS           : CentOS Linux release 7.9.2009 (Core)
CPU          : Intel(R) Core(TM) i7-10700 CPU @ 2.90GHz (8 cores at 3492 MHz)
User         : nmrsu (NMR Administrator (nmrsu))
System       : Avance III 400 NMR spectrometer
1H-frequency : 400.19 MHz
Description  : Avance III 400
Configured in: benmore:/opt/topspin3.6.4/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.90
 - IPSO type: AQS
- Tctrl : 1
- Fctrls: 2
- Gctrl1: without digital preemphasis
- Rctrl : 1
- FREDs : none
- DPP : none

DRU1: AQS DRU Z100977/01160 ECL 05.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x72   0x4    AW  R  4.4 REC-1  AQS RXAD400 Z102116/1556 ECL 04.04
     3   0x34  0x2   0x1        X  5.2 REF-1  REF-400 Reference Board for AQS Receiver
     4   0x24 0x11   0x8    AE  S  2.6 SGU-1  AQS SGU/2 400 Z103080/01678 ECL 02.06 FPGA-Vs=AF
     5   0x25 0x11   0x8    AE  S  2.6 SGU-2  AQS SGU/2 400 Z103080/01679 ECL 02.06 FPGA-Vs=AF
     9   0x36  0x5     0        A  7.0 BLA-1  BLA2BB 150/60 20-400 W1345049/2277 ECL 7
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: 1 AQS-Minirouter

Amplifiers (AQS configuration):
  RO  Amplifier  Module  Nucleus  Power/W  Switchbox Name PN/SN/FW
   1      1         1        B      150    N         BLA2BB 150/60 20-400 W1345049/2277/-
   2      1         2        B       60    N         BLA2BB 150/60 20-400 W1345049/2277/-


Transmitters at the spectrometer subnet:
----------------------------------------
LTRX Z109888/00157 ECL 01.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 400: Z109888/00157 ECL 01.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20210921
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 20
- Shim System = BOSS1-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 400: Z109888/00157 ECL 01.01
- Lock: on L-TRX board

Bruker Automatic Changer: device connected to 149.236.99.90:/dev/tty04
- Capacity: 60 holders
- Firmware: 19990701
- use BACS air  = yes
- BACS sx delay = 10 s
- Sample Rail fast changer mode = no

Eurotherm VTU: device connected to 149.236.99.90:/dev/tty05

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H/2H 1H (virtual 50 Ohm reference: 300.8%/82.7deg)
                PN=Z003959, SN=00704 from 20090821
    Module  2 : 1H/2H 2H (virtual 50 Ohm reference: 98.3%/-69.7deg)
                PN=Z003959, SN=00704 from 20090821
    Module  3 : XBB19F 2HS
                PN=Z003504, SN=00701 from 20090826



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (assumed)
--------------------------------------------------------------------
SGU1 NORM output -> input 2 of transmitter 1 (BLA2BB 150/60 20-400 W1345049/2277)
SGU1 AUX  output -> input 1 of transmitter 2 (BSMS/2 LOCK TRANSCEIVER 400 Z109888/00157 at TCP/IP 149.236.99.20)
SGU2 NORM output -> input 3 of transmitter 1 (BLA2BB 150/60 20-400 W1345049/2277)
SGU2 AUX  output -> TUNE signal input of HPPR

Blanking cable connections (assumed)
--------------------------------------------------------------------
transmitter 1 = BLA2BB 150/60 20-400 W1345049/2277:
- amplifier B-150W uses blanking 1
- amplifier B-60W uses blanking 2

transmitter 2 = BSMS/2 LOCK TRANSCEIVER 400 Z109888/00157 at TCP/IP 149.236.99.20:
- amplifier 2H-5W uses blanking 3


