CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.6.2/conf/instr/spect/uxnmr.info
Date         : Tue Jan 14 16:08:17 2020
Release      : TopSpin 3.6.2
Installed in : C:/Bruker/TopSpin3.6.2
Host         : ERNST
OS           : Windows 7 (Vs 6.2)
CPU          : AMD Ryzen 3 3200G with Radeon Vega Graphics (4 cores at 3593 MHz)
User         : User
System       : Avance III 600 NMR spectrometer
1H-frequency : 600.26 MHz
Description  : Avance III 600
Configured in: ERNST:C:/Bruker/TopSpin3.6.2/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 3
- Gctrl : none
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/01099 ECL 04.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 111024 (needs update to version 170619)
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x62   0x4    AV  R  5.3 REC-1  AQS RXAD-BB Z102119/99 ECL 05.03 (needs update to version AW)
     3   0x34 0xc0   0x1        X  2.0 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x19   0x8    AD  S  2.2 SGU-1  AQS SGU/2 600 Z103081/00884 ECL 02.02 FPGA-Vs=AF
     5   0x25 0x19   0x8    AD  S  2.2 SGU-2  AQS SGU/2 600 Z103081/00889 ECL 02.02 FPGA-Vs=AF
     6   0x26 0x19   0x8    AD  S  2.2 SGU-3  AQS SGU/2 600 Z103081/00892 ECL 02.02 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    23   0x20 0xd1     0        B  2.3 MASTER AQS/3 Chassis
    25   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345088_0057 W1345088/0057 ECL 0:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20100510 (needs update to version 20120627)
- Amplifier      = BLAH1000 E 200-600MHZ: W1345088/0057 ECL 0
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0545 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V V-USB: W1522040/0603 ECL 2
BLA_W1345093_0124 W1345093/0124 ECL 0:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20100510 (needs update to version 20120627)
- Amplifier      = BLAX500 E 6-365MHZ: W1345093/0124 ECL 0
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0522 ECL 0
- Controller     = BLA CONTROL BOARD 6 1V V-USB: W1522041/0342 ECL 2
BLA_W1345095_0100 W1345095/0100 ECL 0:
- TCP/IP address = 149.236.99.251
- Firmware VS    = 20100510 (needs update to version 20120627)
- Amplifier      = BLAX1000 E 6-405MHZ: W1345095/0100 ECL 0
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0548 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V V-USB: W1522040/0596 ECL 2

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20111004
- SCB channels = 40
- Shim System = BOSS-WB
- 2HTX Amplifier: not available
- Lock: not available

MAS2 control unit: connected to 149.236.99.254:/dev/tty01
- Boot Software        : 20031216
- Application Software : 20130613
- Insert Time          : 10 s
- Eject Time           : 10 s
- Spin Lock Tolerance  : 5 Hz

Eurotherm VTU: device connected to 149.236.99.254:/dev/tty05

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : HPHP XBB31P
                PN=Z003549, SN=00061 from 20050331
    Module  2 : HPLNA 1H (virtual 50 Ohm reference: 100.1%/0.0deg, reflection meter)
                PN=Z103205, SN=00010 from 20080124
    Module  3 : HPHP XBB31P
                PN=Z003549, SN=00324 from 20080202
    Module  4 : HPLNA 19F (virtual 50 Ohm reference: 99.7%/-0.2deg, reflection meter)
                PN=Z108964, SN=00001 from 20080327



RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 3 (BLAX1000 E 6-405MHZ W1345095/0100 at TCP/IP 149.236.99.251)
SGU1 AUX  output -> input 2 of transmitter 2 (BLAX500 E 6-365MHZ W1345093/0124 at TCP/IP 149.236.99.252)
SGU2 NORM output -> input 1 of transmitter 1 (BLAH1000 E 200-600MHZ W1345088/0057 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX500 E 6-365MHZ W1345093/0124 at TCP/IP 149.236.99.252)
SGU3 AUX  output -> input 2 of transmitter 1 (BLAH1000 E 200-600MHZ W1345088/0057 at TCP/IP 149.236.99.253)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAH1000 E 200-600MHZ W1345088/0057 at TCP/IP 149.236.99.253:
- amplifier 1H-1000W uses blanking 2
- amplifier 1H-100W uses blanking 2

transmitter 2 = BLAX500 E 6-365MHZ W1345093/0124 at TCP/IP 149.236.99.252:
- amplifier X-500W uses blanking 3

transmitter 3 = BLAX1000 E 6-405MHZ W1345095/0100 at TCP/IP 149.236.99.251:
- amplifier X-1000W uses blanking 1
- amplifier X-300W uses blanking 1


