README: This document describes how to make use of the data used to produce the content of the manuscript, according to the open access regulations enforced by the funder(s). 

TITLE: Photon-sparse microscopy: visible light imaging using infrared illumination 

CREATOR: Reuben Aspden

IDENTIFIER:

DATES: project started August 2013, project ended March 2015, data released November 2015

SUBJECT: Trans-Wavelength imaging, heralded imaging, ghost imaging

FUNDERS: Engineering and Physical Sciences Research Council (EPSRC) and European Research Council (ERC)

RIGHTS: University of Glasgow

METHODOLOGY: The hardware required to reproduce the results - Andor iStar gen III intensifier ICCD, MPD InGaAs/InP SPAD, JDSU Xcyte 355nm 100 mW laser. The software used to run the experiment and generate the data was National Instruments Labview version 2014. The labview project file included in the folder Image Thresholder contains the VI’s necessary to threshold the data used in each of the figures in the paper. The Regulariser_Lambda VI runs in Labview 2014 and was used to optimise the data for the supplementary information.